GPIO requirements

LED Arrays - Power, Ground, 3 GPIO pins(13,11,10) - 5

RF module - Power, Ground, 6 GPIO (refer GitHub wiki)

GY521 - Power, Ground, SDA or A4, SCL or A5.